a. Bit 0 corresponds to board 1, bit 1 corresponds to board 2 and so on.

Action Task

Data Field

11 10 9 8 7 6 5 4 3 2 1 0

Read Interface Housekeeping

0xa Channel Number (0 - 39 decimal)

Read Focal Plane Temperature

0xb -

Read Relay Positions

0xc -

Set Focal Plane Temperature

0x1 12-bit temperature set-point

Set Bakeout Tempearture

0x2 12-bit temperature set-point

Set Spare D/A 0x3 Value

Set CCD Controller Power

0x4 Board Power Selection Mask^a

Discrete Settings 0x5 - - - Hold Hk. Addr.

- - - - - - Bake Out LED

Pulse Actions 0x6 - - - - - - - Reset CCD Controllers

- - - Cal. A/D

Signal Selects 0x7 - - - - Disable Video Clock

Disable 100KHz Synch.

Disable Command Clock

Disable Command Data

- - - Signal Path

Relay Enables 0x8 - - - - - - - R5 R4 R3 R2 R1