TABLE 1. ‘Command Device’ Operations

Function Inputs Outputs Initialize none none Reset Serial Interface none none Install Command Callback Address of function to call when a command packet arrives, the Radiation Monitor Flag is asserted, or an error occurs. This function will be called as part of the Command Interrupt processing.

none

Get Device Status none Current device status Read Command Packet Address of a Command Packet Buffer to copy the data into.

Success, No Packet, or Device Error Read Single Command Word Address of a buffer to copy the word into. Success, No Data, or Device Error Get Radiation Monitor State none Current state of the Radiation Monitor Flag.

TBD: This could be part of “Get Device Status”