TABLE 1. ‘Telemetry Device’ Operations Function Inputs Outputs Initialize none none Install Transfer Complete Callback

Address of function to call whenever a telemetry transfer completes none

Get Device Status none Current device status Send Telemetry Packet Address of Telemetry Packet Buffer to copy data from.

Number of words to transfer.

Success, Busy, or Device Error

Set Discrete Telemetry 4-bit value to write to discrete telemetry bits none