TABLE 1. Telemetry Packet Format

Word # Field Values Description 0 Packet Marker TBD This 32-bit value marks the start of a telemetry packet within the telemetry stream. This value MUST be different from any hardware supplied fill pattern, and from likely values emitted by the hardware when powered off.

1: Bits[0 - 9] Word Count 2 - 1023 This specifies the total number of 32-bit words contained in the telemetry packet, including the “Packet Marker” word.

1: Bits [10-15] Format Tag 1 - TBD The values 0 and 63 are reserved for testing

This field identifies the overall contents and format of the “Data” portion of the telemetry packet.

1: Bits [16 - 31] Sequence Number

0 - 65,535 This field is used to identify the packet in a sequence of packets.

2 - “Word Count” Data Depends on “Format Tag” The remainder of the packet contains the data mandated by the “Format Tag.”