TABLE 1. ‘Telemetry Manager ’ Operations

Function Inputs Outputs Initialize Address of “Telemetry Device” to use for output. none Post Packet Address of the “Telemetry Packet Buffer” to enqueue for transfer out of ACIS.

none

Send Fatal Packet Address of the “Telemetry Packet Buffer” containing the fatal message.

May cause reset of telemetry system.

Get Status none Current status of the telemetry system