time 100KHz Ticks Telemetry Science Frame Pulse Latch and Insert ACIS Timestamp into Telemetry

Increment ACIS Timestamp on each tick

Tell DEA to Start. Sample and store ACIS Timestamp

Send science data containing latched timestamp

Telemetry Science Frame Pulse

Telemetry Science Frame Pulse

Telemetry Science Frame Pulse

Telemetry Science Frame Pulse

Latch and Insert ACIS Timestamp into Telemetry

Latch and Insert ACIS Timestamp into Telemetry

Latch and Insert ACIS Timestamp into Telemetry

Latch and Insert ACIS Timestamp into Telemetry

Clock Pulses Actions