TABLE 1. Discr ete Commands and Flags

Req Name Source Description 1-1 Reset Ground Command This signal resets the ACIS Back End Processor. There is no explicit software monitoring of this signal. This signal will cause ACIS to begin executing its software contained in its Boot ROM.

1-2 Boot Modifier Flag Ground Command When asserted, this signal instructs the ACIS Boot ROM software to load code and data via the Serial Command Channel (Load from Uplink), and to execute the loaded code.

1-3 Science Header Synch S/C Telemetry Clocks

This signal indicates the start of a Science Header Telemetry Frame.

1-4 Radiation Monitor Flag S/C Radiation Moni- tor This signal indicates that the S/C Radiation Monitor has detected a level greater than its current threshold.