TABLE 1. Continue Uplink Load Command Packet Req Item Description 1-1 Packet Length Length of command packet in 16-bit words 1-2 Packet Identifier Used to identify the command 1-3 Command Opcode Continue_Load_Command opcode 1-4 Data to write The data to append to information copied from previous “Start Uplink Load” and possibly “Continue Uplink Load” commands.