TABLE 1. Load DEA Housekeeping List Block Command Packet Req Field Name Description 1-1 Packet Word Length This indicates the total number of 16-bit words in the command packet.

1-2 Packet Identifier This identifies the command packet.

1-3 Command Opcode “Load DEA Housekeeping Parameter Block” command opcode. This instructs the ACIS software to store the List Data contained within the packet.

1-4 Slot Id This identifies the block within ACIS. 1-5 Block CRC or Checksum This is used to check the load.

1-6 Parameter Block Identifier This item is a ground-supplied identifier which is echoed by the instrument software in the DEA housekeeping telemetry.

1-7 Sampling Rate This specifies the rate at which ACIS should sample and telemeter the acquired information. It is specified in terms of number of seconds between item samples. This parameter can range from 1 to 64 seconds.

1-8 DEA Item List The remainder of the packet contains the list of DEA items to sample.