TABLE 1. DEA Housekeeping T elemetry Content

Req Item Description 1-1 Packet Synch This field marks the start of the ACIS packet within the telemetry stream.

1-2 Packet Word

Length

This field indicates the number of 32-bit words in the packet.

1-3 Format Tag This field indicates the type of data contained in the telemetry packet. 1-4 Packet Sequence

Number

This field is used to sequentially number all ACIS telemetry packets.

1-5 Command Packet

Identifier

This is the packet identifier of the start command which initiated the current run.

1-6 BEP Tick Counter This items contains the value of the internal timer-tick counter at approximately the time (i.e. within a minute) when the data contained in the packet was started to be acquired.

1-7 The remainder of the packet contains a list of DEA Housekeeping Entry pairs. The number of entries is determined using the packet length:

1-8 Item Identi- fier This value uniquely identifies the DEA Housekeeping item being sent 1-9 Item Value This is the value of the acquired DEA Housekeeping item.