TABLE 1. Add Bad Pixel Command Packet

Req Item Description 1-1 Packet Length Length of command packet in 16-bit words 1-2 Packet Identifier This is used to identify the command 1-3 Command Opcode Add_Bad_Pixel_Command opcode 1-4 Pixels[Number of entries] This is an array of setting entries. The number of entries is determined using the Packet Length. Each entry has the following format:

1-5 CCD Identifier This specifies the CCD containing the bad pixel.

1-6 Row and Column Addresses

These values identify the row and column within the CCD which is bad, in CCD Coordinates. Summed image pixels which include the specified CCD pixel location are considered bad.