1.

1. Shift down 1 Image and Framestore Row 2. Transfer 1 row out of the Serial Output Shift Registers 3. An X-ray deposits charge in one of the CCD pixels. 4. The charge is transferred to the next row as the CCD is clocked.

5. The charge continues to move down the imaging section into the Framestore.

6. Another X-ray deposits its charge. 7. Eventually, the charge from the first X-ray is clocked from the Framestore into the Serial Output Shift Register 8. The second charge continues to be clocked through the Imaging Section and Framestore to the output register where it is finally read out.

Imaging Section

Framestore Output Registers

Output Nodes

2. 3. 4. 5. 6.

7. 8.

Imaging Section

Framestore Output Registers

Output Nodes