TABLE 1. Bias Map Parity Err or Telemetry Content Req Item Description 1-1 Packet Synch This field marks the start of the ACIS packet within the telemetry stream.

1-2 Packet Word Length This field indicates the number of 32-bit words in the packet. 1-3 Format Tag This field indicates the type of data contained in the telemetry packet, in this case a Timed Exposure Parity Error data packet.

1-4 Packet Sequence Number This field is used to sequentially number all ACIS telemetry packets.

1-5 CCD/FEP Identifiers These identify which CCD and FEP produced the event 1-6 Data Packet Number Since data from different CCDs can be interleaved, and also mixed with other kinds of packets, this field sequentially numbers the parity error packet for a given CCD exposure.

The remainder of the packet contains zero or more of the following:

1-7 Position Identifier This identifies the row and column of the bias error. 1-8 Corrupted Value This a copy of the corrupted pixel bias map value.