Index Description

Min. Value

Max. Value Conversion 0 Parallel Image Array Voltage + 0 TBD Volts = TBD(value) 1 Parallel Image Array Voltage - 0 TBD Volts = TBD(value) 2 Parallel Framestore Voltage + 0 TBD Volts = TBD(value) 3 Parallel Framestore Voltage - 0 TBD Volts = TBD(value) 4 Serial Output Register Voltage + 0 TBD Volts = TBD(value) 5 Serial Output Register Voltage - 0 TBD Volts = TBD(value) 6 Reset Gate Voltage + 0 TBD Volts = TBD(value) 7 Reset Gate Voltage - 0 TBD Volts = TBD(value) 8 Output Gate Voltage 0 TBD Volts = TBD(value) 9 Scupper Voltage 0 TBD Volts = TBD(value) 10 Reset Diode Voltage 0 TBD Volts = TBD(value) 11 Drain Output Channel A Voltage 0 TBD Volts = TBD(value) 12 Drain Output Channel B Voltage 0 TBD Volts = TBD(value) 13 Drain Output Channel C Voltage 0 TBD Volts = TBD(value) 14 Drain Output Channel D Voltage 0 TBD Volts = TBD(value) 15 RTD4 - Board Temperature 0 TBD^οC = TBD(value) 16 RTD3 - SRAM Temperature 0 TBD^οC = TBD(value) 17 RTD2 - ADC Temperature 0 TBD^οC = TBD(value) 18 RTD1 - Gate Array Temperature 0 TBD^οC = TBD(value)