TABLE 1. 2-Dimensional W indow List Parameter Block

Req Item Description 1-1 Parameter Block Identifier

This item is a ground-supplied identifier which is echoed by the instrument software in key portions of the science telemetry.

1-2 Window Count This item identifies the number of 2-D Windows contained in the Window List. This value can range from 0 to 36. This quantity may not actually be loaded nor telemetered, but may be calculated using the length of the enclosing command or telemetry packet.

1-3 Windows[Window Count]

This item is an array of 2-D windows. The content of these windows is described in Table 12. The number of windows in the array is determined by “Window Count.”